<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="5.715" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="7.62" y2="0" width="0" layer="20"/>
<wire x1="7.62" y1="0" x2="8.255" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="8.255" y1="0.635" x2="8.255" y2="5.715" width="0" layer="20"/>
<wire x1="8.255" y1="5.715" x2="7.62" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="7.62" y1="6.35" x2="0.635" y2="6.35" width="0" layer="20"/>
<wire x1="0.635" y1="6.35" x2="0" y2="5.715" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04-1.27MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0402" value="100nF"/>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="RED"/>
<element name="R1" library="adafruit" package="R0603" value="680"/>
<element name="LED2" library="adafruit" package="CHIP-LED0603" value="YELLOW"/>
<element name="R2" library="adafruit" package="R0603" value="680"/>
<element name="IC1" library="adafruit" package="SOT23-6" value="ATTINY10"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04-1.27MM" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04-1.27MM" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="PB2">
<contactref element="IC1" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="5"/>
<contactref element="JP2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="4"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
